/**
  ******************************************************************************
  * @file    readme.txt
  * @author  MCD Application Team
  * @version V4.0.0
  * @date    21-January-2013
  * @brief   Description of the USB Mass_Storage Demo.
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; COPYRIGHT 2013 STMicroelectronics</center></h2>
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
  */


Example description
===================
The Mass Storage Demo gives a typical example of how to use the STM32F10xxx, 
STM32L15xxx , STM32F30xxx and STM32F37xxx USB-FS-Device peripheral to communicate 
with the PC host using the  bulk transfer. 

This demo supports the BOT (bulk only transfer) protocol and all needed SCSI
(small computer system interface) commands, and is compatible with both Windows
XP (SP1/SP2) and Windows 2000 (SP4).

More details about this Demo implementation is given in the User manual 
"UM0424 STM32F10xxx USB development kit", available for download from the ST
microcontrollers website: www.st.com/stm32


Directory contents
==================
 + \inc: contains the Demo firmware header files
 + \EWARM: contains preconfigured projects for EWARM toolchain
 + \RIDE: contains preconfigured projects for RIDE toolchain
 + \MDK-ARM: contains preconfigured projects for MDK-ARM toolchain
 + \TASKING: contains preconfigured projects for TASKING toolchain
 + \TrueSTUDIO: contains preconfigured projects for TrueSTUDIO toolchain          
 + \src: contains the Demo firmware source files


Hardware environment
====================
This example runs these STMicroelectronics evaluation boards and can be easily tailored to any other hardware: 

- STM3210B-EVAL
- STM3210E-EVAL
- STM32L152-EVAL
- STM32F373C_EVAL
- STM32F303C_EVAL
- STM32L152D-EVAL

To select the STMicroelectronics evaluation board used to run the example, uncomment
the corresponding line in platform_config.h file.

  - STM3210B-EVAL Set-up 
     - Jumper JP1 (USB disconnect) should be connected in position 2-3.

  - STM3210E-EVAL Set-up 
     - Jumper JP14 (USB disconnect) should be connected in position 2-3.
     - Jumper JP17 should be connected.
     - Jumper JP20 should be not connected.

  - STM32L152-EVAL Set-up 
     - Jumper JP6 should be connected in position 1-2 (SPI2_MISO side).
     - Jumper JP2 should be not connected.
  
  - STM32L152D-EVAL Set-up 
      - LCD Glass should be mounted On IO position for MicroSD usage.
  
  - STM32F373C_EVAL  Set-up 
      - None.

  - STM32F303C_EVAL  Set-up 
      - None.
    
How to use it
=============
 + EWARM
    - Open the MassStorageSimpleBuffer.eww workspace.
    - In the workspace toolbar select the project config:
        - STM3210B-EVAL: to configure the project for STM32 Medium-density devices
        - STM3210E-EVAL: to configure the project for STM32 High-density devices
        - STM3210E-EVAL_XL: to configure the project for STM32 XL-density devices
        - STM32L152-EVAL: to configure the project for STM32 Medium-Density Low-Power devices
        - STM32L152D-EVAL: to configure the project for STM32 High-Density Low-Power devices
        - STM32373C-EVAL:  to configure the project for STM32F37xxx devices
        - STM32303C-EVAL:  to configure the project for STM32F30xxx devices   
    - Rebuild all files: Project->Rebuild all
    - Load project image: Project->Debug
    - Run program: Debug->Go(F5)

 + MDK-ARM
    - Open the MassStorageSimpleBuffer.Uv2 project
    - In the build toolbar select the project config:
        - STM3210B-EVAL: to configure the project for STM32 Medium-density devices
        - STM3210E-EVAL: to configure the project for STM32 High-density devices
        - STM3210E-EVAL_XL: to configure the project for STM32 XL-density devices
        - STM32L152-EVAL: to configure the project for STM32 Medium-Density Low-Power devices
        - STM32L152D-EVAL: to configure the project for STM32 High-Density Low-Power devices
        - STM32373C-EVAL:  to configure the project for STM32F37xxx devices
        - STM32303C-EVAL:  to configure the project for STM32F30xxx devices   
    - Rebuild all files: Project->Rebuild all target files
    - Load project image: Debug->Start/Stop Debug Session
    - Run program: Debug->Run (F5)

 + RIDE
    - Open the MassStorageSimpleBuffer.rprj project.
    - In the configuration toolbar(Project->properties) select the project config:
        - STM3210B-EVAL: to configure the project for STM32 Medium-density devices
        - STM3210E-EVAL_XL: to configure the project for STM32 XL-density devices
        - STM32L152-EVAL: to configure the project for STM32 Medium-Density Low-Power devices
        - STM32L152D-EVAL: to configure the project for STM32 High-Density Low-Power devices
        - STM32373C-EVAL:  to configure the project for STM32F37xxx devices
        - STM32303C-EVAL:  to configure the project for STM32F30xxx devices  
    - Rebuild all files: Project->build project
    - Load project image: Debug->start(ctrl+D)
    - Run program: Debug->Run(ctrl+F9)

  + TASKING
    - Open TASKING toolchain.
      - Click on File->Import, select General->'Existing Projects into Workspace' 
        and then click "Next". 
      - Browse to TASKING workspace directory and select the project: 
        - STM3210B-EVAL: to configure the project for STM32 Medium-density devices
        - STM3210E-EVAL: to configure the project for STM32 High-density devices
        - STM3210E-EVAL_XL: to configure the project for STM32 XL-density devices
        - STM32L152-EVAL: to configure the project for STM32 Medium-Density Low-Power devices
        - STM32L152D-EVAL: to configure the project for STM32 High-Density Low-Power devices
        - STM32373C-EVAL:  to configure the project for STM32F37xxx devices
        - STM32303C-EVAL:  to configure the project for STM32F30xxx devices   
    - Rebuild all project files: Select the project in the "Project explorer" 
        window then click on Project->build project menu.
    - Run program: Select the project in the "Project explorer" window then click 
        Run->Debug (F11)

 + TrueSTUDIO
    - Open the TrueSTUDIO toolchain.
    - Click on File->Switch Workspace->Other and browse to TrueSTUDIO workspace 
      directory.
    - Click on File->Import, select General->'Existing Projects into Workspace' 
      and then click "Next". 
    - Browse to the TrueSTUDIO workspace directory and select the project:  
        - STM3210B-EVAL: to load the project for STM32 Medium-density devices
        - STM3210E-EVAL: to load the project for STM32 High-density devices
        - STM3210E_EVAL_XL: to load the project for STM32 XL-density devices
        - STM32L152_EVAL: to load the project for STM32 Medium-Density Low-Power devices
        - STM32L152D-EVAL: to configure the project for STM32 High-Density Low-Power devices
        - STM32373C-EVAL:  to configure the project for STM32F37xxx devices
        - STM32303C-EVAL:  to configure the project for STM32F30xxx devices  
    - Rebuild all project files: Select the project in the "Project explorer" 
      window then click on Project->build project menu.
    - Run program: Select the project in the "Project explorer" window then click 
      Run->Debug (F11)

************************ (C) COPYRIGHT STMicroelectronics *****END OF FILE******
